|  |  |  |  |
| --- | --- | --- | --- |
| **GUI ID** | **10-20 Location** | **Wire Color** | New Location |
| -- | Ear Clip  Reference | Black, with white splitter | Cyton Bottom SRB pin (SRB2) |
| 1 | FP1 | Purple | Cyton Bottom N1P pin |
| 2 | FP2 | Gray | Cyton Bottom N2P pin |
| 3 | C3 | Green | Cyton Bottom N4P pin |
| 4 | C4 | Blue | Cyton Bottom N3P pin |
| 5 | P7 | Orange | CP5 |
| 6 | P8 | Yellow | CP6 |
| 7 | O1 | Red | Cyton Bottom N8P pin |
| 8 | O2 | Brown | Cyton Bottom N7P pin |
| -- | Ear Clip -  Digital Ground and noise cancelling | Black | Cyton Bottom BIAS pin |
| -- | Ear Clip -  Reference | Black, with white splitter | Daisy Bottom SRB pin (SRB2) |
| 9 | F7 | Blue | FC1 |
| 10 | F8 | Black | FC2 |
| **11** | **F3** | **White** | **Cz** |
| 12 | F4 | Green | Daisy Bottom N4P pin |
| 13 | T7 | Brown | FC5 |
| 14 | T8 | Red | FC6 |
| 15 | PO3 | Yellow | CP1 |
| 16 | PO4 | Orange | CP2 |